**SANITARY SEWER OVERFLOW (SSO) PUBLIC NOTIFICATION**

**HULL WASTEWATER TREATMENT FACILITY (WWTF)**

in accordance with 314 CMR 16.00

**NOTICE:** The discharge or overflow described in this notification consists, or likely consists, of untreated or partially treated sewage and waste.

Avoid contact with these water bodies for 48 hours after the discharge or overflow ceases due to increased health risks from bacteria and other pollutants. See <https://www.town.hull.ma.us/> for more information on whether specific resource areas, such as bathing beaches, are affected.

For additional information on discharges and overflows, and the Hull WWTF’s SSO Abatement Program, please visit <https://www.town.hull.ma.us/sewer-department/pages/sanitary-sewer-overflow-public-notifications>. You can subscribe to receive E-Alerts at the top of the page.

SSO Event Details

|  |
| --- |
| **Notification Type** |
| **[ ]  Initial-ongoing** | **[x] Initial-ceased** | **[ ] Continuation** | **[ ] Cessation** | **[ ] Retraction** |
| Permitee: Hull Wastewater Treatment Plant | Permit #: MA0101231 |
| **Approximate date and time event began**: Unknown (Approx. 1:00 PM) on 12/11/2023 |
| **Approximate date and time of continuation notice**: NA |
| **Approximate date and time event ceased**: 1:15 PM on 12/11/2023 or [ ] Ongoing |
| **Description of discharge or overflow location(s):**Overflow of primary distribution box due to due to a surge of influent to the plant as a result of rain event. The spillage did not make it to the storm drains or surface water. |
| **Waters and Land Areas, including names of water bodies and municipalities, effected or potentially affected by the discharge or overflow:**From primary distribution box onto adjacent grounds and overland to entrance to cemetery at Spring St.  |
| **Estimate volume of discharge:** | Approximate 200 gallons |